Robotic Fish Command Mode:

1 - Auto Mode by pressing ‘a’

2 - Sensor Values by pressing ‘g’

3 – Resetting everything by pressing ‘z’

4 - Manual Mode by pressing ‘b’

|  |  |
| --- | --- |
| * First Max Angle:   + 1 for 100 degrees   + 2 for 110 degrees   + 3 for 120 degrees   + 4 for 130 degrees   + 5 for 140 degrees   + 6 for 150 degrees   + 7 for 160 degrees | * Second Min Angle:   + 1 for 80 degrees   + 2 for 70 degrees   + 3 for 60 degrees   + 4 for 50 degrees   + 5 for 40 degrees   + 6 for 30 degrees   + 7 for 20 degrees |
| * Third Step size:   + 1 for 1 difference   + 2 for 2 differences   + 3 for 3 differences   + 4 for 4 differences   + 5 for 5 differences   + 6 for 6 differences   + 7 for 7 differences | * Fourth Delay Between Step:   + 1 for 8 seconds   + 2 for 9 seconds   + 3 for 10 seconds   + 4 for 11 seconds   + 5 for 12 seconds   + 6 for 13 seconds   + 7 for 14 seconds |
| * Fifth Delay between each cycle:   + 1 for 2 seconds   + 2 for 3 seconds   + 3 for 4 seconds   + 4 for 5 seconds   + 5 for 6 seconds   + 6 for 7 seconds   + 7 for 8 seconds | |